To install Probe-It wizard, unzip the contents into a folder called ProbeIt.  

Drag the ProbeIt folder into your Mach3 addons folder.  

Most typical installations will be to the following path:
------->    C:\Mach3\Addons\ProbeIt

Requirements:
* You must have Mach3, version 3.43.19 or later.  I recommend the latest lock down or 3.43.66 or later.

* You need to have a probe setup that triggers the 'digitize' input in Mach3.  You may test by assigning a keyboard key to be a 'probe' input if you don't have a probe, but it still requires that you have the parallel port driver installed and an assigned key setup in 'ports and pins'.

* This wizard IS NOT COMPATIBLE with MachStdMill from Calypso Ventures, and cannnot be run while using MachStdMill Screenset due to conflicting use of DROs/LEDs/etc.  A workaround to use this wizard is to setup another Mach3 Profile that uses a standard screenset.

* This wizard is tested to work on machines driven from the standard parallel port, a Smoothstepper, CNCDrive UCx00 (x is any number of their control), or CSMIO.  There is NO guarantee that it will work properly with any other external motion control device, as probing is handled within the motion controllers and not Mach.  Test at your own risk.

* Have some patience in setting up and reading the manual.  If you get stuck, contact me for help 

If interested in unlocking demo-mode with a license, please visit WWW.CraftyCNC.com or email eabrust@craftycnc.com

By installing/using this software, you agree to the terms of the EULA.